1. Section 096813   
   Tile Carpeting
   1. PART 1  GENERAL
      1. SUBMITTALS
         1. See Section 013000 - Administrative Requirements, for submittal procedures.
         2. Samples:  Submit two carpet tiles illustrating color and pattern design for each carpet color selected.
         3. Maintenance Materials:  Furnish the following for Owner's use in maintenance of project.
            1. See Section 016000 - Product Requirements, for additional provisions.
            2. Extra Carpet Tiles:  Quantity equal to 5 percent of total installed of each color and pattern installed.
   2. PART 2  PRODUCTS
      1. MATERIALS
         1. Tile Carpeting​​:  ​Tufted​, manufactured in one color dye lot.
            1. Product:  ​Connected Threads​ manufactured by ​Shaw Contract​.
            2. Style Number:  5T598.
            3. Pattern:  ​Cozy 16111​.
      2. ACCESSORIES
         1. Subfloor Filler:  White premix latex; type recommended by flooring material manufacturer.
         2. Edge Strips:  Embossed aluminum, \_\_\_\_\_ color.
         3. Carpet Tile Adhesive:  Recommended by carpet tile manufacturer; releasable type.
   3. PART 3  EXECUTION
      1. INSTALLATION
         1. Starting installation constitutes acceptance of subfloor conditions.
         2. Install carpet tile in accordance with manufacturer's instructions.
         3. Blend carpet from different cartons to ensure minimal variation in color match.
         4. Cut carpet tile clean.  Fit carpet tight to intersection with vertical surfaces without gaps.
         5. Lay carpet tile in ​Quarter Turn​ pattern, with pile direction ​alternating​ to next unit, set ​parallel to building lines​.
         6. Trim carpet tile neatly at walls and around interruptions.
         7. Complete installation of edge strips, concealing exposed edges.
2. END OF SECTION

This page intentionally left blank